| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
nrf_drv_twi_config_t Struct Reference
TWIS driver

Structure for the TWI master driver instance configuration. More...

`#include <nrf_drv_twi.h>`

## Data Fields
uint32_t | scl
| SCL pin number.
uint32_t | sda
| SDA pin number.
nrf_twi_frequency_t | frequency
| TWI frequency.
uint8_t | interrupt_priority
| Interrupt priority.
bool | clear_bus_init
| Clear bus during init.
bool | hold_bus_uninit
| Hold pull up state on gpio pins after uninit.

## Detailed Description

Structure for the TWI master driver instance configuration.