| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_cts_c_evt_t Struct Reference
Current Time Service client

Current Time Service client event. More...

`#include <ble_cts_c.h>`

## Data Fields
ble_cts_c_evt_type_t | evt_type
uint16_t | conn_handle
union {
current_time_char_t current_time
ble_cts_c_handles_t char_handles
} | params

## Detailed Description

Current Time Service client event.

## Field Documentation

ble_cts_c_handles_t ble_cts_c_evt_t::char_handles

Current Time related handles found on the peer device. This will be filled when the evt_type is BLE_HRS_C_EVT_DISCOVERY_COMPLETE.

uint16_t ble_cts_c_evt_t::conn_handle

Connection handle on which the CTS service was discovered on the peer device. This will be filled if the evt_type is BLE_CTS_C_EVT_DISCOVERY_COMPLETE.

current_time_char_t ble_cts_c_evt_t::current_time

Current Time Characteristic data. This will be filled when the evt_type is BLE_CTS_C_EVT_CURRENT_TIME.

ble_cts_c_evt_type_t ble_cts_c_evt_t::evt_type

Type of event.