| S132 SoftDevice v3.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_gap_sec_levels_t Struct Reference
Structures

Security levels supported. More...

`#include <ble_gap.h>`

## Data Fields
uint8_t | lv1: 1
uint8_t | lv2: 1
uint8_t | lv3: 1
uint8_t | lv4: 1

## Detailed Description

Security levels supported.

Note
  See Bluetooth Specification Version 4.2 Volume 3, Part C, Chapter 10, Section 10.2.1.

## Field Documentation

uint8_t ble_gap_sec_levels_t::lv1

If 1: Level 1 is supported.

uint8_t ble_gap_sec_levels_t::lv2

If 1: Level 2 is supported.

uint8_t ble_gap_sec_levels_t::lv3

If 1: Level 3 is supported.

uint8_t ble_gap_sec_levels_t::lv4

If 1: Level 4 is supported.