| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_ias_c_evt_t Struct Reference
Immediate Alert Service Client

Immediate Alert Service client event. More...

`#include <ble_ias_c.h>`

## Data Fields
ble_ias_c_evt_type_t | evt_type
uint16_t | conn_handle
ble_gattc_char_t | alert_level

## Detailed Description

Immediate Alert Service client event.

## Field Documentation

ble_gattc_char_t ble_ias_c_evt_t::alert_level

Info on the discovered Alert Level characteristic discovered. This will be filled if the evt_type is BLE_IAS_C_EVT_DISCOVERY_COMPLETE.

uint16_t ble_ias_c_evt_t::conn_handle

Connection handle on which the IAS service was discovered on the peer device. This will be filled if the evt_type is BLE_IAS_C_EVT_DISCOVERY_COMPLETE.

ble_ias_c_evt_type_t ble_ias_c_evt_t::evt_type

Type of event.