| S130 SoftDevice v2.0.1 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Macros
GAP Authentication Key Types
Defines

## Macros
#define | BLE_GAP_AUTH_KEY_TYPE_NONE 0x00
#define | BLE_GAP_AUTH_KEY_TYPE_PASSKEY 0x01
#define | BLE_GAP_AUTH_KEY_TYPE_OOB 0x02

## Detailed Description

## Macro Definition Documentation

#define BLE_GAP_AUTH_KEY_TYPE_NONE 0x00

No key (may be used to reject).

#define BLE_GAP_AUTH_KEY_TYPE_OOB 0x02

Out Of Band data.

#define BLE_GAP_AUTH_KEY_TYPE_PASSKEY 0x01

6-digit Passkey.