| S130 SoftDevice v2.0.1 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_gap_opt_passkey_t Struct Reference
Structures

Passkey Option. More...

`#include <ble_gap.h>`

## Data Fields
uint8_t * | p_passkey

## Detailed Description

Passkey Option.

       Structure containing the passkey to be used during pairing. This can be used with @ref
       sd_ble_opt_set to make the SoftDevice use a pre-programmed passkey for authentication
       instead of generating a random one.

Note
  sd_ble_opt_get is not supported for this option.

## Field Documentation

uint8_t* ble_gap_opt_passkey_t::p_passkey

Pointer to 6-digit ASCII string (digit 0..9 only, no NULL termination) passkey to be used during pairing. If this is NULL, the SoftDevice will generate a random passkey if required.