| S130 SoftDevice v2.0.1 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_gatts_authorize_params_t Struct Reference
Structures

GATT Authorization parameters. More...

`#include <ble_gatts.h>`

## Data Fields
uint16_t | gatt_status
uint8_t | update: 1
uint16_t | offset
uint16_t | len
const uint8_t * | p_data

## Detailed Description

GATT Authorization parameters.

## Field Documentation

uint16_t ble_gatts_authorize_params_t::gatt_status

GATT status code for the operation, see GATT Status Codes.

uint16_t ble_gatts_authorize_params_t::len

Length in bytes of the value in p_data pointer, see Maximum attribute lengths.

uint16_t ble_gatts_authorize_params_t::offset

Offset of the attribute value being updated.

const uint8_t* ble_gatts_authorize_params_t::p_data

Pointer to new value used to update the attribute value.

uint8_t ble_gatts_authorize_params_t::update

          If set, data supplied in p_data will be used to update the attribute value.

Please note that for BLE_GATTS_OP_WRITE_REQ operations this bit must always be set, as the data to be written needs to be stored and later provided by the application.