| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
hci_slip_evt_t Struct Reference
SLIP module

Structure containing an event from the SLIP layer. More...

`#include <hci_slip.h>`

## Data Fields
hci_slip_evt_type_t | evt_type
const uint8_t * | packet
uint32_t | packet_length

## Detailed Description

Structure containing an event from the SLIP layer.

## Field Documentation

hci_slip_evt_type_t hci_slip_evt_t::evt_type

Type of event.

const uint8_t* hci_slip_evt_t::packet

This field contains a pointer to the packet for which the event relates, i.e. SLIP_TX_DONE: the packet transmitted, SLIP_RX_RDY: the packet received, SLIP_RX_OVERFLOW: The packet which overflow/or NULL if no receive buffer is available.

uint32_t hci_slip_evt_t::packet_length

Packet length, i.e. SLIP_TX_DONE: Bytes transmitted, SLIP_RX_RDY: Bytes received, SLIP_RX_OVERFLOW: index at which the packet overflowed.