| S132 SoftDevice v3.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
nrf_nvic_state_t Struct Reference
Variables

Type representing the state struct for the SoftDevice NVIC module. More...

`#include <nrf_nvic.h>`

## Data Fields
uint32_t volatile | __irq_masks [__NRF_NVIC_ISER_COUNT]
uint32_t volatile | __cr_flag

## Detailed Description

Type representing the state struct for the SoftDevice NVIC module.

## Field Documentation

uint32_t volatile nrf_nvic_state_t::__cr_flag

Non-zero if already in a critical region

uint32_t volatile nrf_nvic_state_t::__irq_masks[__NRF_NVIC_ISER_COUNT]

IRQs enabled by the application in the NVIC.