| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
nrf_ble_cgms_init_t Struct Reference
Structures

CGM Service initialization structure that contains all options and data needed for initializing the service. More...

`#include <nrf_ble_cgms.h>`

## Data Fields
ble_cgms_evt_handler_t | evt_handler
ble_srv_error_handler_t | error_handler
nrf_ble_cgms_feature_t | feature
nrf_ble_cgm_status_t | initial_sensor_status
uint16_t | initial_run_time

## Detailed Description

CGM Service initialization structure that contains all options and data needed for initializing the service.

## Field Documentation

ble_srv_error_handler_t nrf_ble_cgms_init_t::error_handler

Function to be called when an error occurs.

ble_cgms_evt_handler_t nrf_ble_cgms_init_t::evt_handler

Event handler to be called for handling events in the CGM Service.

nrf_ble_cgms_feature_t nrf_ble_cgms_init_t::feature

Features supported by the service.

uint16_t nrf_ble_cgms_init_t::initial_run_time

Run time.

nrf_ble_cgm_status_t nrf_ble_cgms_init_t::initial_sensor_status

Sensor status.