| S332 SoftDevice v2.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_gap_conn_sec_mode_t Struct Reference
Structures

GAP connection security modes. More...

`#include <ble_gap.h>`

## Data Fields
uint8_t | sm: 4
uint8_t | lv: 4

## Detailed Description

GAP connection security modes.

Security Mode 0 Level 0: No access permissions at all (this level is not defined by the Bluetooth Core specification).
Security Mode 1 Level 1: No security is needed (aka open link).
Security Mode 1 Level 2: Encrypted link required, MITM protection not necessary.
Security Mode 1 Level 3: MITM protected encrypted link required.
Security Mode 1 Level 4: LESC MITM protected encrypted link required.
Security Mode 2 Level 1: Signing or encryption required, MITM protection not necessary.
Security Mode 2 Level 2: MITM protected signing required, unless link is MITM protected encrypted.

## Field Documentation

uint8_t ble_gap_conn_sec_mode_t::lv

Level (1, 2, 3 or 4), 0 for no permissions at all.

uint8_t ble_gap_conn_sec_mode_t::sm

Security Mode (1 or 2), 0 for no permissions at all.