| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_hrs_c_evt_t Struct Reference
Structures

Heart Rate Event structure. More...

`#include <ble_hrs_c.h>`

## Data Fields
ble_hrs_c_evt_type_t | evt_type
uint16_t | conn_handle
union {
hrs_db_t peer_db
ble_hrm_t hrm
} | params

## Detailed Description

Heart Rate Event structure.

## Field Documentation

uint16_t ble_hrs_c_evt_t::conn_handle

Connection handle on which the Heart Rate service was discovered on the peer device..

ble_hrs_c_evt_type_t ble_hrs_c_evt_t::evt_type

Type of the event.

ble_hrm_t ble_hrs_c_evt_t::hrm

Heart rate measurement received. This will be filled if the evt_type is BLE_HRS_C_EVT_HRM_NOTIFICATION.

hrs_db_t ble_hrs_c_evt_t::peer_db

Heart Rate related handles found on the peer device.. This will be filled if the evt_type is BLE_HRS_C_EVT_DISCOVERY_COMPLETE.