| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Public Types | Data Fields
ant_bpwr_sens_cb_t Struct Reference
Bicycle Power profile

Bicycle Power Sensor control block. More...

`#include <ant_bpwr_local.h>`

## Public Types
enum | { BPWR_SENS_CALIB_NONE, BPWR_SENS_CALIB_REQUESTED, BPWR_SENS_CALIB_READY }

## Data Fields
uint8_t | message_counter
ant_bpwr_torque_t | torque_use
enum ant_bpwr_sens_cb_t:: { ... } | calib_stat
ant_bpwr_calib_handler_t | calib_handler

## Detailed Description

Bicycle Power Sensor control block.

## Member Enumeration Documentation

anonymous enum

Enumerator
BPWR_SENS_CALIB_NONE | Idle state.
BPWR_SENS_CALIB_REQUESTED | Received request for general calibration result message by the sensor.
BPWR_SENS_CALIB_READY | Calibration response message is ready to be transmitted.