| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_ans_c_evt_t Struct Reference
Alert Notification Service Client

Alert Notification Event structure. More...

`#include <ble_ans_c.h>`

## Data Fields
ble_ans_c_evt_type_t | evt_type
uint16_t | conn_handle
ble_uuid_t | uuid
union {
ble_ans_alert_settings_t settings
ble_ans_alert_notification_t alert
uint32_t error_code
ble_ans_c_service_t service
} | data

## Detailed Description

Alert Notification Event structure.

The structure contains the event that should be handled, as well as additional information.

## Field Documentation

ble_ans_alert_notification_t ble_ans_c_evt_t::alert

Alert Notification data sent by the server.

uint16_t ble_ans_c_evt_t::conn_handle

Connection handle on which the ANS service was discovered on the peer device. This will be filled if the evt_type is BLE_ANS_C_EVT_DISCOVERY_COMPLETE.

uint32_t ble_ans_c_evt_t::error_code

Additional status/error code if the event was caused by a stack error or gatt status, e.g. during service discovery.

ble_ans_c_evt_type_t ble_ans_c_evt_t::evt_type

Type of event.

ble_ans_c_service_t ble_ans_c_evt_t::service

Info on the discovered Alert Notification Service discovered. This will be filled if the evt_type is BLE_ANS_C_EVT_DISCOVERY_COMPLETE.

ble_ans_alert_settings_t ble_ans_c_evt_t::settings

Setting returned from server on read request.

ble_uuid_t ble_ans_c_evt_t::uuid

UUID of the event in case of an alert or notification.