| S132 SoftDevice v3.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Macros
GAP Keypress Notification Types
Defines

## Macros
#define | BLE_GAP_KP_NOT_TYPE_PASSKEY_START 0x00
#define | BLE_GAP_KP_NOT_TYPE_PASSKEY_DIGIT_IN 0x01
#define | BLE_GAP_KP_NOT_TYPE_PASSKEY_DIGIT_OUT 0x02
#define | BLE_GAP_KP_NOT_TYPE_PASSKEY_CLEAR 0x03
#define | BLE_GAP_KP_NOT_TYPE_PASSKEY_END 0x04

## Detailed Description

## Macro Definition Documentation

#define BLE_GAP_KP_NOT_TYPE_PASSKEY_CLEAR 0x03

Passkey cleared.

#define BLE_GAP_KP_NOT_TYPE_PASSKEY_DIGIT_IN 0x01

Passkey digit entered.

#define BLE_GAP_KP_NOT_TYPE_PASSKEY_DIGIT_OUT 0x02

Passkey digit erased.

#define BLE_GAP_KP_NOT_TYPE_PASSKEY_END 0x04

Passkey entry completed.

#define BLE_GAP_KP_NOT_TYPE_PASSKEY_START 0x00

Passkey entry started.