| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Macros
ANT File Share module. configuration
ANT-FS client device simulator

## Macros
#define | ANTFS_ENABLED
| Set to 1 to activate. More...
#define | ANTFS_CONFIG_NETWORK_NUMBER
| ANT-FS network number. *. More...
#define | ANTFS_CONFIG_CHANNEL_NUMBER
| ANT-FS channel number. *. More...
#define | ANTFS_CONFIG_PAIRING_TIMEOUT
| Pairing timeout - how long the UI will wait for a response to a pairing request before switching to the link layer, in seconds. *. More...
#define | ANTFS_CONFIG_LINK_COMMAND_TIMEOUT
| Command timeout - how long the client will wait without receiving any commands before switching to the link layer, in seconds. *. More...
#define | ANTFS_CONFIG_TRANS_TYPE
| ANT-FS Transmission Type. *. More...
#define | ANTFS_CONFIG_DEVICE_TYPE
| ANT device type for channel configuration. *. More...
#define | ANTFS_CONFIG_BEACON_STATUS_PERIOD
| ANT-FS Beacon Message Period. * Following options are avaiable: More...
#define | ANTFS_CONFIG_TRANSMIT_POWER
| ANT Transmit Power. * Following options are avaiable: More...
#define | ANTFS_CONFIG_CUSTOM_TRANSMIT_POWER
| ANT Custom Transmit Power. *. More...
#define | ANTFS_CONFIG_AUTH_TYPE_PAIRING_ENABLED
| Use pairing and key exchange authentication. * Set to 1 to activate. More...
#define | ANTFS_CONFIG_AUTH_TYPE_PASSKEY_ENABLED
| Use passkey authentication. * Set to 1 to activate. More...
#define | ANTFS_CONFIG_AUTH_TYPE_PASSTHROUGH_ENABLED
| Allow host to bypass authentication. * Set to 1 to activate. More...
#define | ANTFS_CONFIG_UPLOAD_ENABLED
| Support upload operation. * Set to 1 to activate. More...
#define | ANTFS_CONFIG_DEBUG_LED_ENABLED
| Enables LED debug in the module. * Set to 1 to activate. More...

## Detailed Description

## Macro Definition Documentation

#define ANTFS_CONFIG_AUTH_TYPE_PAIRING_ENABLED

Use pairing and key exchange authentication. * Set to 1 to activate.

Note
  This is an NRF_CONFIG macro.

#define ANTFS_CONFIG_AUTH_TYPE_PASSKEY_ENABLED

Use passkey authentication. * Set to 1 to activate.

Note
  This is an NRF_CONFIG macro.

#define ANTFS_CONFIG_AUTH_TYPE_PASSTHROUGH_ENABLED

Allow host to bypass authentication. * Set to 1 to activate.

Note
  This is an NRF_CONFIG macro.

#define ANTFS_CONFIG_BEACON_STATUS_PERIOD

ANT-FS Beacon Message Period. * Following options are avaiable:

- 0 - 0.5 Hz
- 1 - 1 Hz
- 2 - 2 Hz
- 3 - 4 Hz
- 4 - 8 Hz

Note
  This is an NRF_CONFIG macro.

#define ANTFS_CONFIG_CHANNEL_NUMBER

ANT-FS channel number. *.

Note
  This is an NRF_CONFIG macro.

#define ANTFS_CONFIG_CUSTOM_TRANSMIT_POWER

ANT Custom Transmit Power. *.

Note
  This is an NRF_CONFIG macro.

#define ANTFS_CONFIG_DEBUG_LED_ENABLED

Enables LED debug in the module. * Set to 1 to activate.

Note
  This is an NRF_CONFIG macro.

#define ANTFS_CONFIG_DEVICE_TYPE

ANT device type for channel configuration. *.

Note
  This is an NRF_CONFIG macro.

#define ANTFS_CONFIG_LINK_COMMAND_TIMEOUT

Command timeout - how long the client will wait without receiving any commands before switching to the link layer, in seconds. *.

Note
  This is an NRF_CONFIG macro.

#define ANTFS_CONFIG_NETWORK_NUMBER

ANT-FS network number. *.

Note
  This is an NRF_CONFIG macro.

#define ANTFS_CONFIG_PAIRING_TIMEOUT

Pairing timeout - how long the UI will wait for a response to a pairing request before switching to the link layer, in seconds. *.

Note
  This is an NRF_CONFIG macro.

#define ANTFS_CONFIG_TRANS_TYPE

ANT-FS Transmission Type. *.

Note
  This is an NRF_CONFIG macro.

#define ANTFS_CONFIG_TRANSMIT_POWER

ANT Transmit Power. * Following options are avaiable:

- 0 - Lowest ANT Tx power level setting. (-20dBm)
- 1 - ANT Tx power > Lvl 0. (-12dBm)
- 2 - ANT Tx power > Lvl 1. (-4dBm)
- 3 - ANT Tx power > Lvl 2. Default tx power level. (0dBm)
- 4 - ANT Tx power > Lvl 3. (+4dBm)
- 128 - Custom tx power selection

Note
  This is an NRF_CONFIG macro.

#define ANTFS_CONFIG_UPLOAD_ENABLED

Support upload operation. * Set to 1 to activate.

Note
  This is an NRF_CONFIG macro.

#define ANTFS_ENABLED

- Set to 1 to activate.

Note
  This is an NRF_CONFIG macro.