| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Here is a list of all documented struct and union fields with links to the struct/union documentation for each field:

### - p -

- p_adv_burst_config : ant_encrypt_stack_settings_t
- p_alert_msg_buf : ble_ans_alert_notification_t
- p_attr_data : ble_ancs_c_attr_list_t , ble_ancs_c_evt_notif_attr_t
- p_aux_data_ref : nfc_ac_rec_payload_desc_t
- p_bin_pay_desc : nfc_ndef_parser_memo_desc_t
- p_ble_evt : ble_hids_evt_t
- p_body_sensor_location : ble_hrs_init_t
- p_buf : app_fifo_t
- p_buffer : nrf_drv_adc_done_evt_t , nrf_drv_saadc_done_evt_t
- p_cb : ant_bsc_disp_config_t , ant_bsc_sens_config_t , ant_hrm_sens_config_t , ant_sdm_sens_config_t , ant_sdm_disp_config_t , app_mailbox_t , app_pwm_t , ant_bpwr_sens_config_t , ant_bpwr_disp_config_t
- p_char_user_desc : ble_add_char_user_desc_t
- p_chunks : fds_record_t
- p_common : nrf_pwm_values_t
- p_conn_params : ble_conn_params_init_t
- p_context : nrf_drv_timer_config_t , nrf_drv_uart_config_t , fs_evt_t
- p_current_transaction : app_twi_t
- p_data : fds_record_chunk_t , fs_evt_t , app_twi_transfer_t , uint8_array_t , nfc_ac_rec_data_ref_t , nfc_text_rec_payload_desc_t , ble_hids_rep_map_init_t , nrf_drv_uart_xfer_evt_t , fds_flash_record_t
- p_data_dest : ble_ancs_c_t
- p_device_irk : pm_privacy_params_t
- p_encryption_id : ant_encrypt_info_settings_t
- p_end_addr : fs_config_t
- p_ext_rep_ref : ble_hids_rep_map_init_t
- p_feature_rep_array : ble_hids_init_t
- p_file_name : error_info_t , assert_info_t
- p_grouped : nrf_pwm_values_t
- p_header : fds_flash_record_t
- p_id : nfc_ndef_record_desc_t
- p_included_services_array : ble_hids_init_t
- p_individual : nrf_pwm_values_t
- p_init_value : ble_add_char_params_t
- p_inp_rep_array : ble_hids_init_t
- p_instance : nrf_csense_evt_t
- p_lang_code : nfc_text_rec_payload_desc_t
- p_le_data : nrf_crypto_key_t
- p_list : ble_dis_reg_cert_data_list_t , regcertdatalist_t
- p_local_records : nfc_hs_rec_payload_desc_t
- p_location_speed : ble_lns_init_s , ble_lns_s
- p_manuf_specific_data : ble_advdata_t
- p_message_buffer : ble_ans_c_s , ble_ans_c_init_t
- p_msg_desc : nfc_ndef_parser_memo_desc_t
- p_navigation : ble_lns_init_s , ble_lns_s
- p_next : nrf_drv_adc_channel_s , nrf_drv_clock_handler_item_s
- p_operand : ble_racp_value_t , ble_cgms_socp_value_t
- p_outp_rep_array : ble_hids_init_t
- p_pass_key : antfs_params_t
- p_payload : nfc_ndef_bin_payload_desc_t
- p_payload_descriptor : nfc_ndef_record_desc_t
- p_pnp_id : ble_dis_init_t
- p_pool : app_mailbox_t
- p_position_quality : ble_lns_init_s , ble_lns_s
- p_presentation_format : ble_add_char_params_t
- p_primary_buf : nrf_drv_twi_xfer_desc_t
- p_profile : ant_bpwr_simulator_cfg_t , ant_bpwr_simulator_t , ant_bsc_simulator_cfg_t , ant_bsc_simulator_t , ant_hrm_simulator_cfg_t , ant_hrm_simulator_t , ant_sdm_simulator_cfg_t , ant_sdm_simulator_t
- p_qwr : nrf_ble_bms_init_t
- p_random_num_seed : ant_encrypt_info_settings_t
- p_raw : nrf_pwm_values_t
- p_rec_desc : nfc_ndef_parser_memo_desc_t
- p_record : fds_record_desc_t
- p_reg : nrf_drv_rtc_t , nrf_drv_spis_t , nrf_drv_timer_t
- p_reg_cert_data_list : ble_dis_init_t
- p_registers : nrf_drv_pwm_t , nrf_drv_spi_t
- p_remote_friendly_name : antfs_params_t
- p_report_ref : ble_bas_init_t
- p_req : nrf_dfu_req_t
- p_res : nrf_dfu_res_t
- p_rx_buffer : nrf_drv_spi_xfer_desc_t
- p_sec_mgr_oob_flags : ble_advdata_t
- p_secondary_buf : nrf_drv_twi_xfer_desc_t
- p_service_data_array : ble_advdata_t
- p_slave_conn_int : ble_advdata_t
- p_start_addr : fs_config_t
- p_str : ble_srv_utf8_str_t
- p_sys_id : ble_dis_init_t
- p_timer : app_pwm_t
- p_timer_id : low_power_pwm_config_t
- p_tk_value : ble_advdata_t
- p_tlv_block_array : type_2_tag_t
- p_transfers : app_twi_transaction_t
- p_twi : nrf_drv_twi_t
- p_tx_buffer : nrf_drv_spi_xfer_desc_t
- p_tx_power_level : ble_advdata_t
- p_type : nfc_ndef_record_desc_t
- p_uart : nrf_drv_uart_t
- p_user_data : app_twi_transaction_t
- p_user_descr : ble_add_char_params_t
- p_user_info : ant_encrypt_info_settings_t
- p_uuids : ble_advdata_uuid_list_t
- p_value : tlv_block_t , ble_add_descr_params_t
- p_wave_form : nrf_pwm_values_t
- packet : hci_slip_evt_t
- packet_length : hci_slip_evt_t , ant_encrypt_adv_burst_settings_t
- packet_removed_from_tx_fifo : nrf_gzll_host_rx_info_t
- page : fds_reserve_token_t
- page_0 : ant_bsc_profile_s , ant_hrm_profile_s
- page_1 : ant_bpwr_profile_s , ant_bsc_profile_s , ant_hrm_profile_s , ant_sdm_profile_s
- page_16 : ant_bpwr_profile_s
- page_17 : ant_bpwr_profile_s
- page_18 : ant_bpwr_profile_s
- page_1_present : ant_hrm_sens_config_t , ant_bsc_sens_config_t
- page_2 : ant_bsc_profile_s , ant_hrm_profile_s , ant_sdm_profile_s
- page_22 : ant_sdm_profile_s
- page_3 : ant_bsc_profile_s , ant_hrm_profile_s , ant_sdm_profile_s
- page_4 : ant_bsc_profile_s , ant_hrm_profile_s
- page_4_present : ant_bsc_sens_config_t
- page_5 : ant_bsc_profile_s
- page_70 : ant_request_controller_t
- page_80 : ant_bpwr_profile_s , ant_sdm_profile_s
- page_81 : ant_sdm_profile_s , ant_bpwr_profile_s
- page_comb_0 : ant_bsc_profile_s
- page_number : ant_common_page70_data_t
- params : nrf_csense_evt_t
- parity : nrf_drv_uart_config_t
- parse_state : ble_ancs_c_t
- payload_constructor : nfc_ndef_record_desc_t
- payload_length : nfc_ndef_bin_payload_desc_t , nrf_esb_config_t
- payload_received_in_ack : nrf_gzll_device_tx_info_t
- pc : HardFault_stack
- pedal_sensorsim_cfg : ant_bpwr_simulator_cb_t
- pedal_sensorsim_state : ant_bpwr_simulator_cb_t
- peer_bas_db : ble_bas_c_s
- peer_data_update_failed : pm_evt_t
- peer_data_update_succeeded : pm_evt_t
- peer_db : ble_rscs_c_s , ble_hrs_c_evt_t , ble_lbs_c_evt_t
- peer_delete_failed : pm_evt_t
- peer_hrs_db : ble_hrs_c_s
- peer_id : pm_evt_t , pm_peer_data_bonding_t
- peer_lbs_db : ble_lbs_c_s
- peer_ltk : pm_peer_data_bonding_t
- peers_delete_failed_evt : pm_evt_t
- pending_loc_speed_notifications : ble_lns_s
- pending_navigation_notification : ble_lns_s
- pending_racp_response : nrf_ble_cgms_racp_t
- pending_racp_response_operand : nrf_ble_cgms_racp_t
- period : ant_bpwr_page_torque_data_t , low_power_pwm_config_t
- period_us : app_pwm_config_t
- pid : nrf_esb_payload_t
- pin_clk : nrf_drv_pdm_config_t
- pin_din : nrf_drv_pdm_config_t
- pin_no : app_button_cfg_t
- pin_polarity : app_pwm_config_t
- pins : app_pwm_config_t
- pipe : nrf_esb_payload_t
- pos_qual_handles : ble_lns_s
- position_quality_security_req_read_perm : ble_lns_init_s
- position_status : ble_lns_loc_speed_s , ble_lns_pos_quality_s , ble_lns_navigation_s
- positive_action : ble_ancs_c_notif_flags_t
- power_sensorsim_cfg : ant_bpwr_simulator_cb_t
- power_sensorsim_state : ant_bpwr_simulator_cb_t
- pp_key : ant_encrypt_stack_settings_t
- pp_record : nfc_ndef_msg_desc_t
- pre_existing : ble_ancs_c_notif_flags_t
- prescaler : nrf_drv_rtc_config_t
- prev_beat : ant_hrm_page4_data_t
- prev_time_since_evt : ant_bsc_simulator_cb_t
- primary_length : nrf_drv_twi_xfer_desc_t
- priority : fs_config_t
- privacy_mode : pm_privacy_params_t
- private_addr_cycle_s : pm_privacy_params_t
- private_addr_type : pm_privacy_params_t
- procedure : pm_conn_secured_evt_t , pm_conn_secure_failed_evt_t
- procedure_status : ble_sc_ctrlpt_s
- product_id : ble_dis_pnp_id_t
- product_version : ble_dis_pnp_id_t
- progress : nrf_dfu_settings_t
- protocol : nrf_esb_config_t
- protocol_mode_handles : ble_hids_s
- psela : nrf_drv_qdec_config_t
- pselb : nrf_drv_qdec_config_t
- pselcts : nrf_drv_uart_config_t
- pselled : nrf_drv_qdec_config_t
- pselrts : nrf_drv_uart_config_t
- pselrxd : nrf_drv_uart_config_t
- pseltxd : nrf_drv_uart_config_t
- psr : HardFault_stack
- pull : nrf_drv_gpiote_in_config_t
- pull_cfg : app_button_cfg_t
- pulse_rate : ble_bps_meas_s
- pulse_rate_present : ble_bps_meas_s
- push_event : bsp_button_event_cfg_t