| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Command set
This information applies to the nRF52 Series only.

The current version of the NFC Type 2 Tag library supports only one Type 2 Tag command type: the READ command. When a READ command is received, the tag responds with the data that is stored for the tag.

# READ command format

The READ command has the following format:

Byte number | Description | Value
--- | --- | ---
1 | Code | 0x30
2 | Number of the 4-byte data block to read from the tag data | 0x00 - 0xFF

The library can send either a READ response (success) or a NACK response (failure):

- A READ response contains the content of 4 data blocks starting with the requested data block (16 bytes).
- A NACK response contains the error code 0x0, 0x1, 0x4, or 0x5 (4 bits).