| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_rscs_c_evt_t Struct Reference
Running Speed and Cadence Service Client

Running Speed and Cadence Event structure. More...

`#include <ble_rscs_c.h>`

## Data Fields
ble_rscs_c_evt_type_t | evt_type
uint16_t | conn_handle
union {
ble_rscs_c_db_t rscs_db
ble_rsc_t rsc
} | params

## Detailed Description

Running Speed and Cadence Event structure.

## Field Documentation

uint16_t ble_rscs_c_evt_t::conn_handle

Connection handle on which the rscs_c event occured.

ble_rscs_c_evt_type_t ble_rscs_c_evt_t::evt_type

Type of the event.

ble_rsc_t ble_rscs_c_evt_t::rsc

Running Speed and Cadence measurement received. This will be filled if the evt_type is BLE_RSCS_C_EVT_RSC_NOTIFICATION.

ble_rscs_c_db_t ble_rscs_c_evt_t::rscs_db

Running Speed and Cadence Service related handles found on the peer device. This will be filled if the evt_type is BLE_RSCS_C_EVT_DISCOVERY_COMPLETE.