| S132 SoftDevice v3.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Macros
GAP Timeout sources
Defines

## Macros
#define | BLE_GAP_TIMEOUT_SRC_ADVERTISING 0x00
#define | BLE_GAP_TIMEOUT_SRC_SECURITY_REQUEST 0x01
#define | BLE_GAP_TIMEOUT_SRC_SCAN 0x02
#define | BLE_GAP_TIMEOUT_SRC_CONN 0x03
#define | BLE_GAP_TIMEOUT_SRC_AUTH_PAYLOAD 0x04

## Detailed Description

## Macro Definition Documentation

#define BLE_GAP_TIMEOUT_SRC_ADVERTISING 0x00

Advertising timeout.

#define BLE_GAP_TIMEOUT_SRC_AUTH_PAYLOAD 0x04

Authenticated payload timeout.

#define BLE_GAP_TIMEOUT_SRC_CONN 0x03

Connection timeout.

#define BLE_GAP_TIMEOUT_SRC_SCAN 0x02

Scanning timeout.

#define BLE_GAP_TIMEOUT_SRC_SECURITY_REQUEST 0x01

Security request timeout.