| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_nus_c_s Struct Reference
Nordic UART Service Client

NUS Client structure. More...

`#include <ble_nus_c.h>`

## Data Fields
uint8_t | uuid_type
uint16_t | conn_handle
ble_nus_c_handles_t | handles
ble_nus_c_evt_handler_t | evt_handler

## Detailed Description

NUS Client structure.

## Field Documentation

uint16_t ble_nus_c_s::conn_handle

Handle of the current connection. Set with ble_nus_c_handles_assign when connected.

ble_nus_c_evt_handler_t ble_nus_c_s::evt_handler

Application event handler to be called when there is an event related to the NUS.

ble_nus_c_handles_t ble_nus_c_s::handles

Handles on the connected peer device needed to interact with it.

uint8_t ble_nus_c_s::uuid_type

UUID type.