| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_ancs_c_evt_t Struct Reference
Apple Notification Service client

ANCS client module event structure. More...

`#include <ble_ancs_c.h>`

## Data Fields
ble_ancs_c_evt_type_t | evt_type
uint16_t | conn_handle
ble_ancs_c_evt_notif_t | notif
ble_ancs_c_evt_notif_attr_t | attr
ble_ancs_c_service_t | service
uint32_t | error_code

## Detailed Description

ANCS client module event structure.

The structure contains the event that should be handled by the main application.

## Field Documentation

ble_ancs_c_evt_notif_attr_t ble_ancs_c_evt_t::attr

Currently received attribute for a given notification. Will be filled if the evt_type is BLE_ANCS_C_EVT_NOTIF_ATTRIBUTE.

uint16_t ble_ancs_c_evt_t::conn_handle

Connection handle on which the ANCS service was discovered on the peer device. This will be filled if the evt_type is BLE_ANCS_C_EVT_DISCOVERY_COMPLETE.

uint32_t ble_ancs_c_evt_t::error_code

Additional status or error code if the event was caused by a stack error or GATT status, for example, during service discovery.

ble_ancs_c_evt_type_t ble_ancs_c_evt_t::evt_type

Type of event.

ble_ancs_c_evt_notif_t ble_ancs_c_evt_t::notif

iOS notification. Will be filled if evt_type is BLE_ANCS_C_EVT_NOTIF.

ble_ancs_c_service_t ble_ancs_c_evt_t::service

Info on the discovered Alert Notification Service discovered. This will be filled if the evt_type is BLE_ANCS_C_EVT_DISCOVERY_COMPLETE.