| S132 SoftDevice v3.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_gattc_evt_char_val_by_uuid_read_rsp_t Struct Reference
Structures

Event structure for BLE_GATTC_EVT_CHAR_VAL_BY_UUID_READ_RSP. More...

`#include <ble_gattc.h>`

## Data Fields
uint16_t | count
uint16_t | value_len
uint8_t | handle_value [1]

## Detailed Description

Event structure for BLE_GATTC_EVT_CHAR_VAL_BY_UUID_READ_RSP.

## Field Documentation

uint16_t ble_gattc_evt_char_val_by_uuid_read_rsp_t::count

Handle-Value Pair Count.

uint8_t ble_gattc_evt_char_val_by_uuid_read_rsp_t::handle_value[1]

Handle-Value(s) list. To iterate through the list use sd_ble_gattc_evt_char_val_by_uuid_read_rsp_iter.

Note
  This is a variable length array. The size of 1 indicated is only a placeholder for compilation. See sd_ble_evt_get for more information on how to use event structures with variable length array members.

uint16_t ble_gattc_evt_char_val_by_uuid_read_rsp_t::value_len

Length of the value in Handle-Value(s) list.