| S130 SoftDevice v2.0.1 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_gatts_enable_params_t Struct Reference
Structures

BLE GATTS initialization parameters. More...

`#include <ble_gatts.h>`

## Data Fields
uint8_t | service_changed:1
uint32_t | attr_tab_size

## Detailed Description

BLE GATTS initialization parameters.

## Field Documentation

uint32_t ble_gatts_enable_params_t::attr_tab_size

Attribute Table size in bytes. The size must be a multiple of 4. BLE_GATTS_ATTR_TAB_SIZE_DEFAULT is used to set the default size.

uint8_t ble_gatts_enable_params_t::service_changed

Include the Service Changed characteristic in the Attribute Table.