| S132 SoftDevice v3.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_gap_evt_scan_req_report_t Struct Reference
Structures

Event structure for BLE_GAP_EVT_SCAN_REQ_REPORT. More...

`#include <ble_gap.h>`

## Data Fields
int8_t | rssi
ble_gap_addr_t | peer_addr

## Detailed Description

Event structure for BLE_GAP_EVT_SCAN_REQ_REPORT.

## Field Documentation

ble_gap_addr_t ble_gap_evt_scan_req_report_t::peer_addr

             Bluetooth address of the peer device. If the peer_addr resolved: @ref ble_gap_addr_t::addr_id_peer is set to 1

and the address is the device's identity address.

int8_t ble_gap_evt_scan_req_report_t::rssi

Received Signal Strength Indication in dBm.