| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_lncp_mask_t Union Reference
Location and Navigation Service Control Point

A mask can be used to temporarily enable and disable features of the Location and Speed characteristic. More...

`#include <ble_ln_cp.h>`

## Data Fields
uint8_t | flags
struct {
uint8_t instantaneous_speed:1
uint8_t total_distance:1
uint8_t location:1
uint8_t elevation:1
uint8_t heading:1
uint8_t rolling_time:1
uint8_t utc_time:1
}; |

## Detailed Description

A mask can be used to temporarily enable and disable features of the Location and Speed characteristic.