| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Enhanced ShockBurst

Enhanced ShockBurst (ESB) for the nRF5 Series is a simple, lightweight protocol, that is on-air compatible with Nordic's nRF24Lxx devices. ESB for the nRF5 Series provides a simple upgrade path for nRF24Lxx based applications.

The following examples show how to use the ESB protocol:

- Transmitter/Receiver Example
- Low Power Transmitter/Receiver Example