| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_cts_c_init_t Struct Reference
Current Time Service client

Current Time Service client init structure. This structure contains all options and data needed for initialization of the client. More...

`#include <ble_cts_c.h>`

## Data Fields
ble_cts_c_evt_handler_t | evt_handler
ble_srv_error_handler_t | error_handler

## Detailed Description

Current Time Service client init structure. This structure contains all options and data needed for initialization of the client.

## Field Documentation

ble_srv_error_handler_t ble_cts_c_init_t::error_handler

Function to be called if an error occurs.

ble_cts_c_evt_handler_t ble_cts_c_init_t::evt_handler

Event handler to be called for handling events from the Current Time Service client.