| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Macros
Simple application timer functionality configuration
Simple Timer

## Macros
#define | SIMPLE_TIMER_ENABLED
| Enabling simple_timer module * Set to 1 to activate. More...
#define | SIMPLE_TIMER_CONFIG_FREQUENCY
| Timer frequency if in Timer mode * Following options are avaiable: More...
#define | SIMPLE_TIMER_CONFIG_INSTANCE
| TIMER instance used * Following options are avaiable: More...

## Detailed Description

## Macro Definition Documentation

#define SIMPLE_TIMER_CONFIG_FREQUENCY

Timer frequency if in Timer mode * Following options are avaiable:

- 0 - 16 MHz
- 1 - 8 MHz
- 2 - 4 MHz
- 3 - 2 MHz
- 4 - 1 MHz
- 5 - 500 kHz
- 6 - 250 kHz
- 7 - 125 kHz
- 8 - 62.5 kHz
- 9 - 31.25 kHz

Note
  This is an NRF_CONFIG macro.

#define SIMPLE_TIMER_CONFIG_INSTANCE

TIMER instance used * Following options are avaiable:

- 0 - 0
- 1 - 1
- 2 - 2
- 3 - 3 (nRF52 family only)
- 4 - 4 (nRF52 family only)

Note
  This is an NRF_CONFIG macro.

#define SIMPLE_TIMER_ENABLED

Enabling simple_timer module * Set to 1 to activate.

Note
  This is an NRF_CONFIG macro.