| S332 SoftDevice v2.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Structures
Types
Master Boot Record API

## Data Structures
struct | sd_mbr_command_copy_sd_t
| This command copies part of a new SoftDevice The destination area is erased before copying. If dst is in the middle of a flash page, that whole flash page will be erased. If (dst+len) is in the middle of a flash page, that whole flash page will be erased. More...
struct | sd_mbr_command_compare_t
| This command works like memcmp, but takes the length in words. More...
struct | sd_mbr_command_copy_bl_t
| This command copies a new BootLoader. With this command, destination of BootLoader is always the address written in NRF_UICR->BOOTADDR. More...
struct | sd_mbr_command_vector_table_base_set_t
| Sets the base address of the interrupt vector table for interrupts forwarded from the MBR. More...
struct | sd_mbr_command_t

## Detailed Description