| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Macros
SPI Slave driver configuration
SPI slave driver

## Macros
#define | SPIS_ENABLED
| Set to 1 to activate. More...
#define | SPIS_DEFAULT_CONFIG_IRQ_PRIORITY
| Interrupt priority. More...
#define | SPIS_DEFAULT_MODE
| Mode * Following options are avaiable: More...
#define | SPIS_DEFAULT_BIT_ORDER
| SPIS default bit order * Following options are avaiable: More...
#define | SPIS_DEFAULT_DEF
| SPIS default DEF character * Minimum value: 0 Maximum value: 255. More...
#define | SPIS_DEFAULT_ORC
| SPIS default ORC character * Minimum value: 0 Maximum value: 255. More...
#define | SPIS0_ENABLED
| Enable SPIS0 instance * Set to 1 to activate. More...
#define | SPIS1_ENABLED
| Enable SPIS1 instance * Set to 1 to activate. More...
#define | SPIS2_ENABLED
| Enable SPIS2 instance * Set to 1 to activate. More...

## Detailed Description

## Macro Definition Documentation

#define SPIS0_ENABLED

Enable SPIS0 instance * Set to 1 to activate.

Note
  This is an NRF_CONFIG macro.

#define SPIS1_ENABLED

Enable SPIS1 instance * Set to 1 to activate.

Note
  This is an NRF_CONFIG macro.

#define SPIS2_ENABLED

Enable SPIS2 instance * Set to 1 to activate.

Note
  This is an NRF_CONFIG macro.

#define SPIS_DEFAULT_BIT_ORDER

SPIS default bit order * Following options are avaiable:

- 0 - MSB first
- 1 - LSB first

Note
  This is an NRF_CONFIG macro.

#define SPIS_DEFAULT_CONFIG_IRQ_PRIORITY

Interrupt priority.

Priorities 0,2 (nRF51) and 0,1,4,5 (nRF52) are reserved for SoftDevice

Following options are avaiable:

- 0 - 0 (highest)
- 1 - 1
- 2 - 2
- 3 - 3
- 4 - 4 (except nRF51 family)
- 5 - 5 (except nRF51 family)
- 6 - 6 (except nRF51 family)
- 7 - 7 (except nRF51 family)

Note
  This is an NRF_CONFIG macro.

#define SPIS_DEFAULT_DEF

SPIS default DEF character * Minimum value: 0 Maximum value: 255.

Note
  This is an NRF_CONFIG macro.

#define SPIS_DEFAULT_MODE

Mode * Following options are avaiable:

- 0 - MODE_0
- 1 - MODE_1
- 2 - MODE_2
- 3 - MODE_3

Note
  This is an NRF_CONFIG macro.

#define SPIS_DEFAULT_ORC

SPIS default ORC character * Minimum value: 0 Maximum value: 255.

Note
  This is an NRF_CONFIG macro.

#define SPIS_ENABLED

- Set to 1 to activate.

Note
  This is an NRF_CONFIG macro.