| S130 SoftDevice v2.0.1 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Macros
General error codes
BLE SoftDevice Common

General error code definitions for the BLE API. More...

## Macros
#define | BLE_ERROR_NOT_ENABLED (NRF_ERROR_STK_BASE_NUM+0x001)
#define | BLE_ERROR_INVALID_CONN_HANDLE (NRF_ERROR_STK_BASE_NUM+0x002)
#define | BLE_ERROR_INVALID_ATTR_HANDLE (NRF_ERROR_STK_BASE_NUM+0x003)
#define | BLE_ERROR_NO_TX_PACKETS (NRF_ERROR_STK_BASE_NUM+0x004)
#define | BLE_ERROR_INVALID_ROLE (NRF_ERROR_STK_BASE_NUM+0x005)

## Detailed Description

General error code definitions for the BLE API.

## Macro Definition Documentation

#define BLE_ERROR_INVALID_ATTR_HANDLE (NRF_ERROR_STK_BASE_NUM+0x003)

Invalid attribute handle.

#define BLE_ERROR_INVALID_CONN_HANDLE (NRF_ERROR_STK_BASE_NUM+0x002)

Invalid connection handle.

#define BLE_ERROR_INVALID_ROLE (NRF_ERROR_STK_BASE_NUM+0x005)

Invalid role.

#define BLE_ERROR_NO_TX_PACKETS (NRF_ERROR_STK_BASE_NUM+0x004)

Not enough application packets available on this connection.

#define BLE_ERROR_NOT_ENABLED (NRF_ERROR_STK_BASE_NUM+0x001)

sd_ble_enable has not been called.