| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
BSP NFC Module

You can use the NFC BSP Module to set the NFCT peripheral as a wakeup source. It can be used with other BSP modules as long as their button configuration is not overwritten by this module.

The application must notify this module before going into System OFF mode. Based on this notification, the NFC BSP Module sets the NFCT peripheral as a wakeup source through the Board Support Package.

Additionally, the NFC Module can configure any BSP Button to generate BSP sleep events.

Note that this module is applicable only if NFCT is used exclusively for wakeup. If NFCT is used for a different purpose (e.g. URI Message Example), this module cannot be used.