| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_hts_meas_s Struct Reference
Health Thermometer Service

Health Thermometer Service measurement structure. This contains a Health Thermometer measurement. More...

`#include <ble_hts.h>`

## Data Fields
bool | temp_in_fahr_units
bool | time_stamp_present
bool | temp_type_present
ieee_float32_t | temp_in_celcius
ieee_float32_t | temp_in_fahr
ble_date_time_t | time_stamp
uint8_t | temp_type

## Detailed Description

Health Thermometer Service measurement structure. This contains a Health Thermometer measurement.

## Field Documentation

ieee_float32_t ble_hts_meas_s::temp_in_celcius

Temperature Measurement Value (Celcius).

ieee_float32_t ble_hts_meas_s::temp_in_fahr

Temperature Measurement Value (Fahrenheit).

bool ble_hts_meas_s::temp_in_fahr_units

True if Temperature is in Fahrenheit units, Celcius otherwise.

uint8_t ble_hts_meas_s::temp_type

Temperature Type.

bool ble_hts_meas_s::temp_type_present

True if Temperature Type is present.

ble_date_time_t ble_hts_meas_s::time_stamp

Time Stamp.

bool ble_hts_meas_s::time_stamp_present

True if Time Stamp is present.