| S332 SoftDevice v2.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_evt_data_length_changed_t Struct Reference
Structures

Event structure for BLE_EVT_DATA_LENGTH_CHANGED. More...

`#include <ble.h>`

## Data Fields
uint16_t | max_tx_octets
uint16_t | max_tx_time
uint16_t | max_rx_octets
uint16_t | max_rx_time

## Detailed Description

Event structure for BLE_EVT_DATA_LENGTH_CHANGED.

## Field Documentation

uint16_t ble_evt_data_length_changed_t::max_rx_octets

The maximum number of payload octets in a Link Layer Data Channel PDU that the local controller expects to receive. Range: 27-251

uint16_t ble_evt_data_length_changed_t::max_rx_time

The maximum time (in microseconds) that the local Controller expects to take to receive a Link Layer Data Channel PDU. Range: 328-2120

uint16_t ble_evt_data_length_changed_t::max_tx_octets

The maximum number of payload octets in a Link Layer Data Channel PDU that the local Controller will send. Range: 27-251

uint16_t ble_evt_data_length_changed_t::max_tx_time

The maximum time (in microseconds) that the local Controller will take to send a Link Layer Data Channel PDU. Range: 328-2120