| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
led_sb_init_params_t Struct Reference
LED softblink

Structure holding the initialization parameters. More...

`#include <led_softblink.h>`

## Data Fields
bool | active_high
uint8_t | duty_cycle_max
uint8_t | duty_cycle_min
uint8_t | duty_cycle_step
uint32_t | off_time_ticks
uint32_t | on_time_ticks
uint32_t | leds_pin_bm

## Detailed Description

Structure holding the initialization parameters.

## Field Documentation

bool led_sb_init_params_t::active_high

Activate negative polarity.

uint8_t led_sb_init_params_t::duty_cycle_max

Maximum impulse width.

uint8_t led_sb_init_params_t::duty_cycle_min

Minimum impulse width.

uint8_t led_sb_init_params_t::duty_cycle_step

Cycle step.

uint32_t led_sb_init_params_t::leds_pin_bm

Mask of used LEDs.

uint32_t led_sb_init_params_t::off_time_ticks

Ticks to stay in low impulse state.

uint32_t led_sb_init_params_t::on_time_ticks

Ticks to stay in high impulse state.