| S332 SoftDevice v2.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_gap_adv_ch_mask_t Struct Reference
Structures

Channel mask for RF channels used in advertising. More...

`#include <ble_gap.h>`

## Data Fields
uint8_t | ch_37_off: 1
uint8_t | ch_38_off: 1
uint8_t | ch_39_off: 1

## Detailed Description

Channel mask for RF channels used in advertising.

## Field Documentation

uint8_t ble_gap_adv_ch_mask_t::ch_37_off

Setting this bit to 1 will turn off advertising on channel 37

uint8_t ble_gap_adv_ch_mask_t::ch_38_off

Setting this bit to 1 will turn off advertising on channel 38

uint8_t ble_gap_adv_ch_mask_t::ch_39_off

Setting this bit to 1 will turn off advertising on channel 39