| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
TX Power Service
This information applies to the following SoftDevices: S130, S132, S332

This module implements the TX Power Service with the TX Power Level characteristic. During initialization it adds the TX Power Service and TX Power Level characteristic with the specified initial value to the BLE stack database.

It provides a function for letting the application update the TX Power Level characteristic.