| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
nrf_drv_twis_config_t Struct Reference
TWIS driver

Structure for TWIS configuration. More...

`#include <nrf_drv_twis.h>`

## Data Fields
uint32_t | addr [2]
| Set addresses that this slave should respond. Set 0 to disable.
uint32_t | scl
| SCL pin number.
nrf_gpio_pin_pull_t | scl_pull
| SCL pin pull.
uint32_t | sda
| SDA pin number.
nrf_gpio_pin_pull_t | sda_pull
| SDA pin pull.
uint8_t | interrupt_priority
| The priority of interrupt for the module to set.

## Detailed Description

Structure for TWIS configuration.