| S130 SoftDevice v2.0.1 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Modules | Macros
Defines
Logical Link Control and Adaptation Protocol (L2CAP)

## Modules
| SVC return values specific to L2CAP

## Macros
#define | BLE_L2CAP_MTU_DEF (23)
| Default L2CAP MTU.
#define | BLE_L2CAP_CID_INVALID (0x0000)
| Invalid Channel Identifier.
#define | BLE_L2CAP_CID_DYN_BASE (0x0040)
| Dynamic Channel Identifier base.
#define | BLE_L2CAP_CID_DYN_MAX (8)
| Maximum amount of dynamic CIDs.

## Detailed Description