| S130 SoftDevice v2.0.1 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Macros
GAP Scan window max and min
Defines

## Macros
#define | BLE_GAP_SCAN_WINDOW_MIN 0x0004
#define | BLE_GAP_SCAN_WINDOW_MAX 0x4000

## Detailed Description

## Macro Definition Documentation

#define BLE_GAP_SCAN_WINDOW_MAX 0x4000

Maximum Scan window in 625 us units, i.e. 10.24 s.

#define BLE_GAP_SCAN_WINDOW_MIN 0x0004

Minimum Scan window in 625 us units, i.e. 2.5 ms.