| S132 SoftDevice v3.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Macros
GAP Connection Parameters Limits
Defines

## Macros
#define | BLE_GAP_CP_MIN_CONN_INTVL_NONE 0xFFFF
#define | BLE_GAP_CP_MIN_CONN_INTVL_MIN 0x0006
#define | BLE_GAP_CP_MIN_CONN_INTVL_MAX 0x0C80
#define | BLE_GAP_CP_MAX_CONN_INTVL_NONE 0xFFFF
#define | BLE_GAP_CP_MAX_CONN_INTVL_MIN 0x0006
#define | BLE_GAP_CP_MAX_CONN_INTVL_MAX 0x0C80
#define | BLE_GAP_CP_SLAVE_LATENCY_MAX 0x01F3
#define | BLE_GAP_CP_CONN_SUP_TIMEOUT_NONE 0xFFFF
#define | BLE_GAP_CP_CONN_SUP_TIMEOUT_MIN 0x000A
#define | BLE_GAP_CP_CONN_SUP_TIMEOUT_MAX 0x0C80

## Detailed Description

## Macro Definition Documentation

#define BLE_GAP_CP_CONN_SUP_TIMEOUT_MAX 0x0C80

Highest supervision timeout permitted, in units of 10 ms, i.e. 32 s.

#define BLE_GAP_CP_CONN_SUP_TIMEOUT_MIN 0x000A

Lowest supervision timeout permitted, in units of 10 ms, i.e. 100 ms.

#define BLE_GAP_CP_CONN_SUP_TIMEOUT_NONE 0xFFFF

No new supervision timeout specified in connect parameters.

#define BLE_GAP_CP_MAX_CONN_INTVL_MAX 0x0C80

Highest maximum connection interval permitted, in units of 1.25 ms, i.e. 4 s.

#define BLE_GAP_CP_MAX_CONN_INTVL_MIN 0x0006

Lowest maximum connection interval permitted, in units of 1.25 ms, i.e. 7.5 ms.

#define BLE_GAP_CP_MAX_CONN_INTVL_NONE 0xFFFF

No new maximum connection interval specified in connect parameters.

#define BLE_GAP_CP_MIN_CONN_INTVL_MAX 0x0C80

Highest minimum connection interval permitted, in units of 1.25 ms, i.e. 4 s.

#define BLE_GAP_CP_MIN_CONN_INTVL_MIN 0x0006

Lowest minimum connection interval permitted, in units of 1.25 ms, i.e. 7.5 ms.

#define BLE_GAP_CP_MIN_CONN_INTVL_NONE 0xFFFF

No new minimum connection interval specified in connect parameters.

#define BLE_GAP_CP_SLAVE_LATENCY_MAX 0x01F3

Highest slave latency permitted, in connection events.