| S130 SoftDevice v2.0.1 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Macros
GAP Address cycle modes
Defines

## Macros
#define | BLE_GAP_ADDR_CYCLE_MODE_NONE 0x00
#define | BLE_GAP_ADDR_CYCLE_MODE_AUTO 0x01

## Detailed Description

## Macro Definition Documentation

#define BLE_GAP_ADDR_CYCLE_MODE_AUTO 0x01

Automatically generate and update private addresses.

#define BLE_GAP_ADDR_CYCLE_MODE_NONE 0x00

Set addresses directly, no automatic address cycling.