| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Macros
PWM peripheral driver configuration
PWM driver

## Macros
#define | PWM_ENABLED
| Set to 1 to activate. More...
#define | PWM_DEFAULT_CONFIG_OUT0_PIN
| Out0 pin * Minimum value: 0 Maximum value: 31. More...
#define | PWM_DEFAULT_CONFIG_OUT1_PIN
| Out1 pin * Minimum value: 0 Maximum value: 31. More...
#define | PWM_DEFAULT_CONFIG_OUT2_PIN
| Out2 pin * Minimum value: 0 Maximum value: 31. More...
#define | PWM_DEFAULT_CONFIG_OUT3_PIN
| Out3 pin * Minimum value: 0 Maximum value: 31. More...
#define | PWM_DEFAULT_CONFIG_BASE_CLOCK
| Base clock * Following options are avaiable: More...
#define | PWM_DEFAULT_CONFIG_COUNT_MODE
| Count mode * Following options are avaiable: More...
#define | PWM_DEFAULT_CONFIG_TOP_VALUE
| Top value *. More...
#define | PWM_DEFAULT_CONFIG_LOAD_MODE
| Load mode * Following options are avaiable: More...
#define | PWM_DEFAULT_CONFIG_STEP_MODE
| Step mode * Following options are avaiable: More...
#define | PWM_DEFAULT_CONFIG_IRQ_PRIORITY
| Interrupt priority. More...
#define | PWM0_ENABLED
| Enable PWM0 instance * Set to 1 to activate. More...
#define | PWM1_ENABLED
| Enable PWM1 instance * Set to 1 to activate. More...
#define | PWM2_ENABLED
| Enable PWM2 instance * Set to 1 to activate. More...

## Detailed Description

## Macro Definition Documentation

#define PWM0_ENABLED

Enable PWM0 instance * Set to 1 to activate.

Note
  This is an NRF_CONFIG macro.

#define PWM1_ENABLED

Enable PWM1 instance * Set to 1 to activate.

Note
  This is an NRF_CONFIG macro.

#define PWM2_ENABLED

Enable PWM2 instance * Set to 1 to activate.

Note
  This is an NRF_CONFIG macro.

#define PWM_DEFAULT_CONFIG_BASE_CLOCK

Base clock * Following options are avaiable:

- 0 - 16 MHz
- 1 - 8 MHz
- 2 - 4 MHz
- 3 - 2 MHz
- 4 - 1 MHz
- 5 - 500 kHz
- 6 - 250 kHz
- 7 - 125 MHz

Note
  This is an NRF_CONFIG macro.

#define PWM_DEFAULT_CONFIG_COUNT_MODE

Count mode * Following options are avaiable:

- 0 - Up
- 1 - Up and Down

Note
  This is an NRF_CONFIG macro.

#define PWM_DEFAULT_CONFIG_IRQ_PRIORITY

Interrupt priority.

Priorities 0,1,4,5 (nRF52) are reserved for SoftDevice

Following options are avaiable:

- 0 - 0 (highest)
- 1 - 1
- 2 - 2
- 3 - 3
- 4 - 4
- 5 - 5
- 6 - 6
- 7 - 7

Note
  This is an NRF_CONFIG macro.

#define PWM_DEFAULT_CONFIG_LOAD_MODE

Load mode * Following options are avaiable:

- 0 - Common
- 1 - Grouped
- 2 - Individual
- 3 - Waveform

Note
  This is an NRF_CONFIG macro.

#define PWM_DEFAULT_CONFIG_OUT0_PIN

Out0 pin * Minimum value: 0 Maximum value: 31.

Note
  This is an NRF_CONFIG macro.

#define PWM_DEFAULT_CONFIG_OUT1_PIN

Out1 pin * Minimum value: 0 Maximum value: 31.

Note
  This is an NRF_CONFIG macro.

#define PWM_DEFAULT_CONFIG_OUT2_PIN

Out2 pin * Minimum value: 0 Maximum value: 31.

Note
  This is an NRF_CONFIG macro.

#define PWM_DEFAULT_CONFIG_OUT3_PIN

Out3 pin * Minimum value: 0 Maximum value: 31.

Note
  This is an NRF_CONFIG macro.

#define PWM_DEFAULT_CONFIG_STEP_MODE

Step mode * Following options are avaiable:

- 0 - Auto
- 1 - Triggered

Note
  This is an NRF_CONFIG macro.

#define PWM_DEFAULT_CONFIG_TOP_VALUE

Top value *.

Note
  This is an NRF_CONFIG macro.

#define PWM_ENABLED

- Set to 1 to activate.

Note
  This is an NRF_CONFIG macro.