| S332 SoftDevice v2.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_common_opt_conn_evt_ext_t Struct Reference
Structures

Configuration of extended BLE connection events. More...

`#include <ble.h>`

## Data Fields
uint8_t | enable: 1

## Detailed Description

Configuration of extended BLE connection events.

When enabled the SoftDevice will dynamically extend the connection event when possible.

The connection event length is controlled by the bandwidth configuration as set by ble_common_opt_conn_bw_t. The connection event can be extended if there is time to send another packet pair before the start of the next connection interval, and if there are no conflicts with other BLE roles requesting radio time.

Note
  sd_ble_opt_get is not supported for this option.

## Field Documentation

uint8_t ble_common_opt_conn_evt_ext_t::enable

Enable extended BLE connection events, disabled by default.