| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
nrf_drv_gpiote_out_config_t Struct Reference
GPIOTE driver

Output pin configuration. More...

`#include <nrf_drv_gpiote.h>`

## Data Fields
nrf_gpiote_polarity_t | action
nrf_gpiote_outinit_t | init_state
bool | task_pin

## Detailed Description

Output pin configuration.

## Field Documentation

nrf_gpiote_polarity_t nrf_drv_gpiote_out_config_t::action

Configuration of the pin task.

nrf_gpiote_outinit_t nrf_drv_gpiote_out_config_t::init_state

Initial state of the output pin.

bool nrf_drv_gpiote_out_config_t::task_pin

True if the pin is controlled by a GPIOTE task.