| S130 SoftDevice v2.0.1 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_gap_evt_connected_t Struct Reference
Structures

Event structure for BLE_GAP_EVT_CONNECTED. More...

`#include <ble_gap.h>`

## Data Fields
ble_gap_addr_t | peer_addr
ble_gap_addr_t | own_addr
uint8_t | role
uint8_t | irk_match:1
uint8_t | irk_match_idx:7
ble_gap_conn_params_t | conn_params

## Detailed Description

Event structure for BLE_GAP_EVT_CONNECTED.

## Field Documentation

ble_gap_conn_params_t ble_gap_evt_connected_t::conn_params

GAP Connection Parameters.

uint8_t ble_gap_evt_connected_t::irk_match

If 1, peer device's address resolved using an IRK.

uint8_t ble_gap_evt_connected_t::irk_match_idx

Index in IRK list where the address was matched.

ble_gap_addr_t ble_gap_evt_connected_t::own_addr

Bluetooth address of the local device used during connection setup.

ble_gap_addr_t ble_gap_evt_connected_t::peer_addr

Bluetooth address of the peer device.

uint8_t ble_gap_evt_connected_t::role

BLE role for this connection, see GAP Roles