| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Data Fields
ble_hids_rep_map_init_t Struct Reference
Human Interface Device Service

HID Service Report Map characteristic init structure. This contains all options and data needed for initialization of the Report Map characteristic. More...

`#include <ble_hids.h>`

## Data Fields
uint8_t * | p_data
uint16_t | data_len
uint8_t | ext_rep_ref_num
ble_uuid_t * | p_ext_rep_ref
ble_srv_security_mode_t | security_mode

## Detailed Description

HID Service Report Map characteristic init structure. This contains all options and data needed for initialization of the Report Map characteristic.

## Field Documentation

uint16_t ble_hids_rep_map_init_t::data_len

Length of report map data.

uint8_t ble_hids_rep_map_init_t::ext_rep_ref_num

Number of Optional External Report Reference descriptors.

uint8_t* ble_hids_rep_map_init_t::p_data

Report map data.

ble_uuid_t* ble_hids_rep_map_init_t::p_ext_rep_ref

Optional External Report Reference descriptor (will be added if != NULL).

ble_srv_security_mode_t ble_hids_rep_map_init_t::security_mode

Security mode for the HID Service Report Map characteristic.