| S130 SoftDevice v2.0.1 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
Macros
Module specific SVC, event and option number subranges
BLE SoftDevice Common

Definition of SVC, event and option number subranges for each API module. More...

## Macros
#define | BLE_SVC_BASE 0x60
#define | BLE_SVC_LAST 0x6B
#define | BLE_RESERVED_SVC_BASE 0x6C
#define | BLE_RESERVED_SVC_LAST 0x6F
#define | BLE_GAP_SVC_BASE 0x70
#define | BLE_GAP_SVC_LAST 0x8F
#define | BLE_GATTC_SVC_BASE 0x90
#define | BLE_GATTC_SVC_LAST 0x9F
#define | BLE_GATTS_SVC_BASE 0xA0
#define | BLE_GATTS_SVC_LAST 0xAF
#define | BLE_L2CAP_SVC_BASE 0xB0
#define | BLE_L2CAP_SVC_LAST 0xBF
#define | BLE_EVT_INVALID 0x00
#define | BLE_EVT_BASE 0x01
#define | BLE_EVT_LAST 0x0F
#define | BLE_GAP_EVT_BASE 0x10
#define | BLE_GAP_EVT_LAST 0x2F
#define | BLE_GATTC_EVT_BASE 0x30
#define | BLE_GATTC_EVT_LAST 0x4F
#define | BLE_GATTS_EVT_BASE 0x50
#define | BLE_GATTS_EVT_LAST 0x6F
#define | BLE_L2CAP_EVT_BASE 0x70
#define | BLE_L2CAP_EVT_LAST 0x8F
#define | BLE_OPT_INVALID 0x00
#define | BLE_OPT_BASE 0x01
#define | BLE_OPT_LAST 0x1F
#define | BLE_GAP_OPT_BASE 0x20
#define | BLE_GAP_OPT_LAST 0x3F
#define | BLE_GATTC_OPT_BASE 0x40
#define | BLE_GATTC_OPT_LAST 0x5F
#define | BLE_GATTS_OPT_BASE 0x60
#define | BLE_GATTS_OPT_LAST 0x7F
#define | BLE_L2CAP_OPT_BASE 0x80
#define | BLE_L2CAP_OPT_LAST 0x9F

## Detailed Description

Definition of SVC, event and option number subranges for each API module.

Note
  SVCs, event and option numbers are split into subranges for each API module. Each module receives its entire allocated range of SVC calls, whether implemented or not, but return BLE_ERROR_NOT_SUPPORTED for unimplemented or undefined calls in its range.

Note that the symbols BLE_<module>_SVC_LAST is the end of the allocated SVC range, rather than the last SVC function call actually defined and implemented.

Specific SVC, event and option values are defined in each module's ble_<module>.h file, which defines names of each individual SVC code based on the range start value.

## Macro Definition Documentation

#define BLE_EVT_BASE 0x01

Common BLE Event base.

#define BLE_EVT_INVALID 0x00

Invalid BLE Event.

#define BLE_EVT_LAST 0x0F

Total: 15.

#define BLE_GAP_EVT_BASE 0x10

GAP BLE Event base.

#define BLE_GAP_EVT_LAST 0x2F

Total: 32.

#define BLE_GAP_OPT_BASE 0x20

GAP BLE Option base.

#define BLE_GAP_OPT_LAST 0x3F

Total: 32.

#define BLE_GAP_SVC_BASE 0x70

GAP BLE SVC base.

#define BLE_GAP_SVC_LAST 0x8F

Total: 32.

#define BLE_GATTC_EVT_BASE 0x30

GATTC BLE Event base.

#define BLE_GATTC_EVT_LAST 0x4F

Total: 32.

#define BLE_GATTC_OPT_BASE 0x40

GATTC BLE Option base.

#define BLE_GATTC_OPT_LAST 0x5F

Total: 32.

#define BLE_GATTC_SVC_BASE 0x90

GATTC BLE SVC base.

#define BLE_GATTC_SVC_LAST 0x9F

Total: 32.

#define BLE_GATTS_EVT_BASE 0x50

GATTS BLE Event base.

#define BLE_GATTS_EVT_LAST 0x6F

Total: 32.

#define BLE_GATTS_OPT_BASE 0x60

GATTS BLE Option base.

#define BLE_GATTS_OPT_LAST 0x7F

Total: 32.

#define BLE_GATTS_SVC_BASE 0xA0

GATTS BLE SVC base.

#define BLE_GATTS_SVC_LAST 0xAF

Total: 16.

#define BLE_L2CAP_EVT_BASE 0x70

L2CAP BLE Event base.

#define BLE_L2CAP_EVT_LAST 0x8F

Total: 32.

#define BLE_L2CAP_OPT_BASE 0x80

L2CAP BLE Option base.

#define BLE_L2CAP_OPT_LAST 0x9F

Total: 32.

#define BLE_L2CAP_SVC_BASE 0xB0

L2CAP BLE SVC base.

#define BLE_L2CAP_SVC_LAST 0xBF

Total: 16.

#define BLE_OPT_BASE 0x01

Common BLE Option base.

#define BLE_OPT_INVALID 0x00

Invalid BLE Option.

#define BLE_OPT_LAST 0x1F

Total: 31.

#define BLE_RESERVED_SVC_BASE 0x6C

Reserved BLE SVC base.

#define BLE_RESERVED_SVC_LAST 0x6F

Total: 4.

#define BLE_SVC_BASE 0x60

Common BLE SVC base.

#define BLE_SVC_LAST 0x6B

Total: 12.