| nRF5 SDK v12.0.0 |

Choose documentation: | nRF5 SDK | S130 SoftDevice API | S132 SoftDevice API | S212 SoftDevice API | S332 SoftDevice API

All Data Structures Functions Variables Typedefs Enumerations Enumerator Groups Pages
LED Softblink Example

The LED Softblink Example demonstrates how to use the LED softblink library. It shows how to light up the LEDs with a gradual changing intensity that depends on the parameters that are specified during initialization.

You can find the source code and the project file of the example in the following folder: `<InstallFolder>\examples\peripheral\led_softblink`

# Testing

Test the LED Softblink Example application by performing the following steps:

1. Compile and program the application.
2. Observe that the LED light intensity changes. The LEDs stay turned off for 2 seconds between every cycle.